org.cloudbus.cloudsim.power.models (cloudsim 3.1-SNAPSHOT API)

# Package org.cloudbus.cloudsim.power.models

- Interface Summary
  Interface | Description
  --- | ---
  PowerModel | The PowerModel interface needs to be implemented in order to provide a model of power consumption depending on utilization for system components.

- Class Summary
  Class | Description
  --- | ---
  PowerModelCubic | The Class PowerModelCubic.
  PowerModelLinear | The Class PowerModelLinear.
  PowerModelSpecPower | The abstract class of power models created based on data from SPECpower benchmark: http://www.spec.org/power_ssj2008/ If you are using any algorithms, policies or workload included in the power package, please cite the following paper: Anton Beloglazov, and Rajkumar Buyya, "Optimal Online Deterministic Algorithms and Adaptive Heuristics for Energy and Performance Efficient Dynamic Consolidation of Virtual Machines in Cloud Data Centers", Concurrency and Computation: Practice and Experience, ISSN: 1532-0626, Wiley Press, New York, USA, 2011, DOI: 10.1002/cpe.1867
  PowerModelSpecPower_BAZAR | PowerModel for REIMS GRID 5000 SITE.
  PowerModelSpecPower_BAZAR_MultiProc | PowerModel for Tom's Host.
  PowerModelSpecPower_REIMS | PowerModel for Tom's Host.
  PowerModelSpecPower_REIMS_Disk | PowerModel for Tom's Host.
  PowerModelSpecPower_REIMS_Net | PowerModel for Tom's Host.
  PowerModelSpecPowerDVFS | Generic Power Model Class Using DVFS Your PowerModel class (with yours power consumption values must extend this class
  PowerModelSpecPowerHpProLiantMl110G3PentiumD930 | The power model of an HP ProLiant ML110 G3 (1 x [Pentium D930 3000 MHz, 2 cores], 4GB).
  PowerModelSpecPowerHpProLiantMl110G4Xeon3040 | The power model of an HP ProLiant ML110 G4 (1 x [Xeon 3040 1860 MHz, 2 cores], 4GB).
  PowerModelSpecPowerHpProLiantMl110G5Xeon3075 | The power model of an HP ProLiant ML110 G5 (1 x [Xeon 3075 2660 MHz, 2 cores], 4GB).
  PowerModelSpecPowerIbmX3250XeonX3470 | The power model of an IBM server x3250 (1 x [Xeon X3470 2933 MHz, 4 cores], 8GB).
  PowerModelSpecPowerIbmX3250XeonX3480 | The power model of an IBM server x3250 (1 x [Xeon X3480 3067 MHz, 4 cores], 8GB).
  PowerModelSpecPowerIbmX3550XeonX5670 | The power model of an IBM server x3550 (2 x [Xeon X5670 2933 MHz, 6 cores], 12GB).
  PowerModelSpecPowerIbmX3550XeonX5675 | The power model of an IBM server x3550 (2 x [Xeon X5675 3067 MHz, 6 cores], 16GB).
  PowerModelSqrt | The Class PowerModelSqrt.
  PowerModelSquare | The Class PowerModelSquare.

Copyright © 2013 The Cloud Computing and Distributed Systems (CLOUDS) Laboratory, The University of Melbourne. All Rights Reserved.